Guide to installing OS/2 Warp Server Backup/Restore (PSnS) Corrective Service
=============================================================================

To check what level of PSnS you have installed, you can run the commnand 
"syslevel" from an OS/2 prompt and look for the output from the file
SYSLEVEL.PSS.  Alternatively, you can select "Help" and "Product information"
from the action bar of the PSnS user interface.

Corrective service diskettes (CSDs) are provided here as diskette images.
There are separate sets of diskettes for different languages and for different  
fix levels.  We did not produce corrective service in all languages.  You
cannot apply corrective service for one language to another.

Some corrective service fits onto a single diskette, others need two diskettes.
The diskette image file names are the CSD names, with extensions of DK1 or DK2.
For example, the files for English CSD 3009014 are 3009014.DK1 and 3009014.DK2.

The first, or only, diskette of a CSD has a README.1ST file and a file with
the name of the (English) CSD and an extension of INF that may be viewed with
the VIEW program.  For example, type "view a:\3009014.inf" to view the
information for CSD 3009014.  The INF file will give details of each APAR
fixed in that CSD, as well as more information on applying corrective service.

To install a CSD you will need a service tool diskette.  We provide this as a
diskette image file with an extension of DSK.  There are a number of these
images at different levels.  We say which level we tested each CSD with.

To run the service tool, place the diskette in a drive and type "a:\service"
at an OS/2 command prompt.  The utility will ask for the (first) corrective
service diskette (CSD).  Follow the on-screen prompts.

In order to make diskettes from these image files, the utility program
LOADDSKF.EXE is provided.  Executing this program with no parameters will
give you help on how to use it.  All images are for 1.44MB diskettes.

Here is a list of all the CSDs on this site.  The most recent are at the top:

-----------------

CSD:      30x9104
Version:  6.00.2
FixTool:  CS_140.DSK

English:   3009104.DK1, 3009104.DK2 
Brazilian: 30B9104.DK1, 30B9104.DK2
French:    30F9104.DK1
Japanese:  30J9104.DK1, 30J9102.DK2

NOTE:  This CSD does NOT provide service for the Backup/Restore component of
OS/2 Warp Server for e-business.

-----------------

CSD:      30x9102
Version:  6.00.1
FixTool:  CS_139.DSK

English:   3009102.DK1
Brazilian: 30B9102.DK1
German:    30G9102.DK1
Japanese:  30J9102.DK1, 30J9102.DK2

-----------------

CSD:      30x9016
Version:  5.02.1
FixTool:  SERVICE.DSK

English:   3009016.DK1, 3009016.DK2
German:    30G9016.DK1, 30G9016.DK2
Japanese:  30J9016.DK1, 30J9016.DK2

-----------------

CSD:      30x9015
Version:  5.02.0
FixTool:  SERVICE.DSK

Brazilian: 30B9015.DK1, 30B9015.DK2
Italian:   30I9015.DK1, 30I9015.DK2
Japanese:  30J9015.DK1, 30J9015.DK2

-----------------

CSD:      30x9014
Version:  5.01.7
FixTool:  SERVICE.DSK

English:   3009014.DK1, 3009014.DK2
French:    30F9014.DK1, 30F9014.DK2
German:    30G9014.DK1, 30G9014.DK2
Japanese:  30J9014.DK1, 30J9014.DK2
