Figure 17. Sample CONFIG.DFM File

     ; ************************************************************************
     ; * Delete or comment out the lines not needed (i.e., add a ';' in front).
     ; * Uncomment lines you want activated (i.e., delete the ';' in front).
     ; * Modify the values as required.
     ; ************************************************************************

     ; ************************************************************************
     ; * Define all DFM/2 target systems on which you want to access file data.
     ; ************************************************************************
     ; The name specified in the remote_lu parameter of the DFM_TARGET
     ; statement connects the definition to the partner_lu_alias specification
     ; of a DEFINE_PARTNER_LU statement in the node definitions file for the
     ; OS/2 Communications Manager (the configuration.NDF file normally
     ; residing in c:\cmlib\appn).

     ; Definition of an MVS system as target:
            DFM_TARGET (
                  remote_lu(TLBA07ME)
                  description(your MVS System)
                  conversation(HOLD)
                  max_send_limit(4096)
                  userid(youruser)
                  )

     ; ************************************************************************
     ; * Define local LU alias as defined for the OS/2 Communications Mgr.
     ; ************************************************************************
            LOCAL_LU (ELNQF0EA)

     ; ************************************************************************
     ; * Define the Mode Name
     ; ************************************************************************
            MODE_NAME (QPCSUPP)

     ; ************************************************************************
     ; * Define the Default DFM Target System
     ; ************************************************************************
     ;       DEFAULT_DFM_TARGET(OS400M1)

     ; ************************************************************************
     ; * Define default CCSID (Coded-Character-Set-Id, up to 5 decimal digits)
     ; * for all accessed targets:
     ; * Some examples for CCSIDs (code pages)
     ; * (CEPC means EBCDIC format, PC Data means ASCII format):
     ; * 037 = CEPC: USA, Canada (ESA), Netherlands, Portugal, Brazil, Australia
     ; * 273 = CEPC: Austria, Germany
     ; * 277 = CEPC: Denmark, Norway
     ; * 278 = CEPC: Finland, Sweden
     ; * 280 = CEPC: Italy
     ; * 284 = CEPC: Spain, Latin America (Spanish)
     ; * 285 = CEPC: United Kingdom
     ; * 297 = CEPC: France
     ; * 500 = CEPC: International Latin-1, B, CH, Can(AS/400)  (default)
     ; * 437 = PC Data: USA
     ; * 850 = PC Data: Latin Alphabet Number 1, Latin-1 Countries
     ; ************************************************************************
            DEFAULT_CCSID(00500)