;Input file for MKMSGF the resulting .MSG file must be placed in the DPATH or 
;the template file specification must specify the path on the boot drive.
;
;The 'number' component of the msg id must be 4 numeric chars.
;This 'number' is what is used in the template file _causes _actions phrases
;between the comma's. e.g. Fail Causes = 4,5,0,0 will cause SYSLOG to display 
;message BNB0004I followed by BNB0005I in its fail causes section. 
;Message text can continue across multiple lines if so desired. 
BNB
BNB0001I: Message for probe 11111, with 2 substitution vars: %1 and %2
BNB0002I: Message for probe 22222, with 2 substitution vars: %1 and %2
BNB0003I: Hello World!
BNB0004I: Hello World! My_Dummy_API returned a non-zero rc
BNB0005I: A non-zero rc is the result of 123456 not being sent to My_Dummy_API
BNB0006I: Call My_Dummy_API with 123456 passed as Mydata.
BNB0007I: Is the Log User Data sent with this probe, formatted to hexidecimal
BNB0008I: Is the Log User Data sent with this probe, formatted to ASCII
BNB0009I: Is the Log User Data sent with this probe, formatted as decimal
